|  |  |
| --- | --- |
| Izpolni naročnik – organizator prevoza / To be filled out by client | **KONTROLNI LIST PRED NAKLADANJEM NEVARNEGA BLAGA – V EMBALAŽI**CHECK FORM BEFORE LOADING DANGEROUS GOODS – PACKAGED V KOLIKOR JE NA PREVOZNI ENOTI ŽE NALOŽENO NEVARNO BLAGO – UPOŠTEVATI ZAHTEVE O DOPUSTNEM SKUPNEM NAKLADANJUIN CASE THE TRANSPORT UNIT IS ALREADY LOADED WITH DANGEROUS GOODS - RESPECT THE REQUIREMENTS ON ALLOWABLE MIXED LOADINGA. SPLOŠNI PODATKI1. Registrska št. vozila/ priklopnika \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Registration no. vehicle/trailer2. Voznik (ime in priimek) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Driver (name and surname)3. UN številka/razred /embalažna skupina \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ UN number/class/packing group (navedite podatke ali priložite fotokopijo CMR listine /  provide information or attach a photocopy of the CMR list)4. Količina naloženega nevarnega blaga PO SPREMLJAJOČI DOKUMENTACIJI Amount of loaded dangerous goods ACCORDING TO ACCOMPANYING DOCUMENTATION5. Št. izhodne dispozicije (DIZ) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ No. of output dispositionB. KONTROLA DOKUMENTOV IN VOZILA 1. Certifikat ADR o usposobljenosti voznika \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Drivers certificate of ADR competence 2. Listina o prevozu nevarnega blaga DA NE – blago v omejenih količinah Document on the transport of dangerous goods NO – goods  NAROČNIK CUSTOMER/CLIENTKraj in datum \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_ /\_\_\_ / 20\_\_\_ Place and date |
| Izpolni voznik / driver | C. POTRJUJEM:Da vozilo ustreza zahtevam za prevoz nevarnega blaga (oprema vozila, oranžne table in nalepke nevarnosti). V kabini vozila so pisna navodila po ADR. I CERTIFY:That the vehicle meets the requirements for the transport of dangerous goods (equipment, orange-coloured plates and placards). There are instructions in writing according to ADR in the cabin of the vehicle. VOZNIKDRIVER   |